LoRa.

The connection to the Gateway is successful with the pi. The code used to run this is radio\_receiver.py The guide to run it can be found here: <https://github.com/ronoth/LoStik>

The Nodes were not working though, documentation said that the nodes reset by putting the magnet over the cover, but this did not end up working. The gateway wasn’t receiving any information from it either.

Note that to run the script you have to open the terminal and run ./radio\_receiver.py /dev/ttyUSB0.

The connection to the website as described in the documentation papers provided with the gateway/nodes was not successful, because the login credentials were not working. I contacted P Kengen about this twice, but he answered the other questions, and didn’t send the login credentials.